**HORSE WEIGH ASSEMBLY INSTRUCTIONS**

**Tokyo**

|  |  |  |
| --- | --- | --- |
|  **E** |  **P** |  **E** |

 **Key**

 **E end section**

 **P platform central section**

1. Please refer to the Golden Rules that were inside the lid of your Tokyo kit box.
2. The three sections will clip together underneath the platform, by using the auto-locating catches.
3. Draw the blue cables out to one side, and attach them to the indicator (weight read-out unit). Make sure that the caps are screwed together so that no dust or damp can get in to them. The handler can pick up the indicator once the horse is on the platform or an assistant can hold it.

For any other queries contact Horse Weigh®

Tel +44 (0) 7774 783247 or +44 (0)1939 220669 william@horseweigh.com

**HORSE WEIGH ASSEMBLY INSTRUCTIONS**

**Tokyo – Thoroughbred**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  **R** |  **E** |  **P** |  **E** |  **R** |

 **Key**

 **R ramp**

 **E end section**

 **P platform central section**

1. Please refer to the Tokyo- Thoroughbred Golden Rules that are inside the lid of your Tokyo -Thoroughbred kit box
2. Assemble as above, as for the Tokyo, and add the ramps at each end.
3. To join the three pieces of each guide rail you will need the allen key (black hexagonal key) which is stored in the lid of the box, behind the Golden Rules. Please make sure that each rail is assembled with its marked friend’s with 1s and 2s with 2s. Once assembled, take off the bottom nut. The rails will now drop into the holes in the platform. Replace nut on the underside. The top nut must be tight at all times. Both nuts, above and below, tighten left to right (anti-clockwise).

1. The blue cables can be drawn out from under the platform and connected to the indicator, (weight read-out unit) which is attached to the board on the guide rail.
2. Please make sure that the feet of the platform are **not** on top of the blue

cables.

 For all other queries contact Horse Weigh®

 Tel +44 (0) 7774 783247 or +44 (0)1939 220669 william@horseweigh.com